
Steps to take to install a driver for a HEPC8, HEPC3,
HEPC4 or HECPCI1 board on Windows 95/98:

If you already inserted the board, then Windows 95/98
will have told you it found new hardware. 

If you have not yet installed the board, shutdown your
computer and insert the board. When Windows starts up
and detects the new hardware choose ignore when it asks 
for the drivers.

After the board is inserted do the following.

1. Start up the Hardware Wizard:

      - Start->Settings->Control Panel
      - Double click on "Add New Hardware"

2. You will see the "Add new Hardware Wizard" window.

      - Click "Next"

3. If you are asked whether to search for new hardware or 
the drivers. It is not necessary to search.


4. You will be asked what hardware you want to install

      - Scroll the sidebar downwards,
      - then select "Other devices".
      - Click "Next"

5. You will be asked to select Manufacturer and Model of
   the hardware.

      - Click "Have Disk"

6. You will see the "Install from Disk" window.

      - Type the name of the directory where you installed
        the Hunt Engineering API into (or use "Browse" to
        browse to the same directory).
      - The file needed is "hunteng.inf", but you should
        =NOT= specify this, only the directory.
      - Click "OK"

7. Now you should see a screen saying the following:

        HEPC2E Rev B/C
        HEPC2E Rev B/C, without Jtag
        HEPC3 Rev B/C
        HEPC6 Rev A
        HEPC6 Rev A, without Jtag
        HEPC8 Rev A

   Select the board for which you wish to install the
   driver. If you have a HEPC4 or HECPCI1, select HEPC3.
   (Since for these 3 boards the interface is exactly the
   same, they all use the same driver.)

      - Select your board.
      - Click "Next"

8. Now you will see a screen that tells you whether
   Windows can install the driver. If Windows says
   it can install the driver,

      - Click "Next"

   If Windows says it cannot install the driver, you
   can (1) quit the installation or (2) continue to
   install the driver. Either way, you will have to
   find the reason of the resource conflict. If you
   install the driver, it will be installed properly
   but will not function properly (as Windows cannot
   start it up since other drivers use resources also
   claimed by the Hunt Engineering board driver).

9. You may see a screen saying that "hepxxui.dll"
   could not be found (where xx is 2e, 3b, 6a or 8a).

      - Click "OK"

   should solve this.

10. You will see a screen that tells you that the
    driver installation is finished.

      - Click "Finish"

11. OK, the driver is installed. Now some parameters need
    to be changed. Start up the driver panel as follows:

      - Start->Settings->Control Panel
      - Double click on "System"

12. The "System Properties" window will appear.

      - Click the "Device Manager" tab.
      - Click on the "+" before "HuntEngClass".
      - Select the board that you just installed.
      - Double click this board

13. The property page of the driver will appear.

      - Click the "Driver" tab.
      - Check that the driver files it lists are 	
    	c:\windows\system\hep8aui.dll
   	c:\windows\system\hep8avxd.dll
	if not then
      		- Click on "Change Driver"
  
 		   Windows lists the driver you just installed.

	      	- Click "OK"
      		- You will now see two Driver files:

		c:\windows\system\hep8aui.dll
    		c:\windows\system\hep8avxd.dll

      		- Click "OK"
      - Click the "Options" tab 
        (If you had to do the "Change Driver" option, you must
         first "OK", then again double click on the board.)

      - There are 4 options here.

           MAKE SURE THAT MASTERMODE IS SWITCHED OFF!

14. Close the "System Properties" window.

      - Click "Close"

15. Now please do the confidence checks.

This completes the installation.
