
File Menu:
  [Interrupt Test (HEPC8 only)] This confidence test verifies whether
  interrupts are enabled or disabled.  If enabled, it checks whether
  the interrupt works properly.
  [Reads Test] This confidence test verifies if proper data can
  be read from the board. It only works if a processor module is
  inserted in slot 1.
  [Writes Test] This confidence test verifies if data can be
  written properly to the board. It only works if a processor
  module is inserted in slot 1.
  [Idrom Test (C4x only)] This confidence test verifies that a
  TIM-40 IDROM can be read properly. It only works if a processor
  module is inserted in slot 1.

Options Menu:
  [Board Type] Selects the board on which to execute the confidence
  checks in the File Menu.
  [Board Number] Selects the board number of the board on which
  to execute the confidence checks in the File Menu, in case you
  installed more than 1 identical board.
  [Comport] Selects the comport for the board on which to execute
  the confidence checks in the File Menu.
  [R/W Settings] Selects the buffer start/end/increment sizes for
  the File Menu's Reads and Writes Test.
  [Show JTAG regs] When doing a JTAG Reset in the Tools Menu, you
  can select whether to have the contents of 16 JTAG registers dumped.

Tools Menu:
  [Board Reset] Resets the board (as selected under the Options Menu).
  [JTAG Reset] Resets the JTAG of the board (as selected under the
  Options Menu)

Registry Menu:
  [Refresh] This is a dynamic menu. With Refresh this menu can be
  updated when drivers get installed or un-installed.
  [HEP8A 0/1/2/3] If present, allows you to change the settings of the HEPC8 driver.
  [HEP6A 0/1/2/3] If present, allows you to change the settings of the HEPC6 driver.
  [HEP3B 0/1/2/3] If present, allows you to change the settings of the HEPC3 driver.
  [HEP2E 0/1/2/3] If present, allows you to change the settings of the HEPC2 driver.

Help Menu:
  [About] About chat.
  [Help] This file.


