
API & Tools 1.9.15 (may 27, 2008)
  * Updated 64-bit driver for HEPC9

API & Tools 1.9.14 (september 25, 2007)
  * SDP version 2.09
  * Host API version 1.9.11

API & Tools 1.9.13 (march 26, 2007)
  * SDP version 2.08

API & Tools 1.9.12 (july 10, 2006)
  * Removed API JTAG reset from start up and screen
  * Removed AutoConfigure CCS from install and screen
  * Host API version 1.9.9b (HERON-BASE2 driver update)
  * hrn_fpga 2.7
  * SDP version 2.07

API & Tools 1.9.11 (september 15, 2005)
  * Host API version 1.9.9 (HERON-BASE2 support added)
  * confchk version 1.9.10 (HERON-BASE2 support added)
  * hrn_fpga 2.6
  * SDP version 2.05 (includes SL 4.13) (HERON-BASE2 support)

API & Tools 1.9.10 (may 11, 2005)
  * confchk version 1.9.9
  * hrn_fpga 2.5
  * RTOS32 hrn_fpga updated to 2.5
  * SDP version 2.04 (includes SL 4.12)

API & Tools 1.9.9 (september 2, 2004)
  * confchk version 1.9.8
  * hrn_fpga 2.4

API & Tools 1.9.8 (april 27, 2004)
  * Host API version 1.9.8
  * SDP version 2.03 (includes SL 4.11)
  * API 1.9.8, SL 4.11 support for VXWORKS
  * API 1.9.8, SL 4.11 support for RTOS-32

API & Tools 1.9.7 (december 16, 2003)
  * Host API version 1.9.7
  * confchk version 1.9.7
  * SDP version 2.02
  * API 1.9.7, SL 4.10 support for LINUX
    (for RedHat 6.1, 7.1 and 9.0)

API & Tools 1.9.6 (november 25, 2003)
  * Host API version 1.9.6
  * confchk version 1.9.6
  * SDP version 2.01

API & Tools 1.9.5 (june 12, 2003)
  * Confchk version 1.9.5.
  * host API version 1.9.5 (HEPC9 LINUX support added)
  * SDP changed to C6000 SDP in install.

API & Tools 1.9.4 (may 13, 2003)
  * Confchk version 1.9.4.
  * Host API version 1.9.4.
  * Two missing HERON2 files from HERON-API added to installation
    (heron2_bios.cmd, heron2_slbios.cmd).

API & Tools 1.9.3 (april 25, 2003)
  * Confchk version 1.9.3.
  * Host API version 1.9.3
  * Software Developer's Pack 2.0.
  * Multiple board support, multiple board install.
  * Environment variables changed to registry entries.
  * Install now installs boards with any boardswitch setting.
  * Component install, former seperate API and SDP install
    merged into one.
  
API & Tools 1.9.2 (march 18, 2003)
  * HCB support added. Affects confchk only.
  * Utility hrn_fpga now works with hcb (compressed rbt) and rbt

API & Tools 1.9.1 (november 26, 2002)
  * HERON2 support added. Affects confchk only.
    HeartConf now automatically upgrades heron-id
    where board bits are 0.

API & Tools 1.9.0 (september 30, 2002)
  * WDM support added for Windows 2000 and XP:
       HEPC9, HEPC8, HEPC3 (but not for HEPC2E)
  * WDM drivers replace NT's kdd drivers used until now
    on Windows 2000 and XP.
  * WDM drivers not yet tested on multi-processor PC's.

API & Tools 1.8.7 (july 4, 2002)
  * HeartConf now supports EM1C, EM1, EM2.
  * Confidence checks upgraded.

API & Tools 1.8.6 (may 22, 2002)
  * VxWorks support updated to work with HEPC8.
    VxWorks support for HEPC8 bug fix (concurrent read/write)

API & Tools 1.8.5 (may 13, 2002)
  * Heartconf problem fixed. Didn't handle properly some
    'overlapping' heart connections.

API & Tools 1.8.4 (may 7, 2002)
  * Confchk problem with C6201 fixed

API & Tools 1.8.3 (april 26, 2002)
  * AutoConfig plug-in upgraded for CCS 2.1

API & Tools 1.8.2 (march 22, 2002)
  * NT driver crash fixed

API & Tools 1.8.1 (march 6, 2002)
  * final HEPC9 API
     - interrupts supported
     - master mode implemented
    Some issues remain:
     - multi threading not 100% reliable
     - NT driver crashes if cancelling ongoing transfer
  * updated utils

API & Tools 1.8.0 (june 28, 2001)
  * preliminary version for IDC 2001
  * HEPC9 support added
     - no interrupts yet
     - no mastermode yet

API & Tools 1.7.1 (june 20, 2001)
  * Updated to accommodate CCS v. 2.0
    - confchk.exe: autoconfig feature will now copy
      CDB files according to the CCS version.
    - confchk.exe: autoconfig feature will remove
      all other boards before adding Hunt board.

API & Tools 1.7.0 (april 09, 2001)

  * FPGA based confidence check added.
  * FPGA only install is now possible.
  * RTOS-32 support added.
  * Confchk, heprojct plug-in and uninst changed to understand
    multiple CCS installations. CCS may still not work though
    as it may fall over its own legs.
  * Heprojct plug-in can now also use *.C files as project names;
    the project name is derived from the C file name (no ext.)
  * Resetsys plug-in: bug fix (edit C file, recompile problem).
  * Resetsys plug-in: tracing is now an option (default: off)

API & Tools 1.6.4 (july 12, 2001)

  * LINUX only!!!
  * Support for RedHat Linux 7.1 added. Now installs on both
    RedHat Linux 6.1 and 7.1

API & Tools 1.6.3 (february 13, 2001)

  * All I2C references changed to HSB
  * Uninstall now also deletes plug-in *.dat files

API & Tools 1.6.2 (december 05, 2000)

  * Confchk.exe changed to allow new drivers or driver 
    updates use the same name ("HUNT ENGINEERING API")

API & Tools 1.6.1 (november 30, 2000)

  * New CCS driver added (tixds6000.dvr 3.15)

API & Tools 1.6.0 (october 13, 2000)

  * This version will install and work under W2000. However,
    currently PnP is bypassed, so at every reboot the machine
    will complain that it found new hardware. You can ignore
    this, the drivers are installed and work, but W2000 just
    doesn't understand there really is a driver there.
  * New driver for Code Composer Studio added. The new driver
    solves problems that occurred with HEPC8 systems having
    more than 3 processors onboard. 
  * Serial bus support added to the API, updated files are:
    - hendrv.dll, hendrv.lib
    - hebdrv.dll, hebdrv.lib
    - hep8avxd.vxd
    - hep8akdd.sys
    - heapi.h
    - hecodes.c, hecodes.h
    Serial bus allows applications to automatically check what
    HERON type a certain module is, e.g. HERON1 or HERON4
  * Serial bus support added to the confidence check program
    - confchk.exe 1.6.1
  * Create new project plug-in updated. (1) Previously always
    file "stub.c" was added to Server/Loader projects. But if
    there's more than 1 project in a directory, this can cause
    problems. New plug-in creates a unique name for the stub
    file, so that you can have any number of stub files for
    any number of projects in the same directory. 
    (2) When creating an SL project, the new project plug-in
    will also add a template network file and a w32.bat file.
    (3) When adding an existing C file, the new project plug-in
    will verify that the heron include file matches the heron
    module type the project is set up for.
    (4) If the C file added has no bootloader() call even while
    a new project for the S/L is created, a warning is given.
    (5) Gconfgen is now used to generate the *.s62 and *.h62
    files. The created project is ready-to-compile, but be
    careful as no tasks/threads have been added!!!!
    - heprojct.ocx 1.3.1
  * MS-DOS examples / confidence checks updated to work with HERON4
    and the serial bus.
    - c6x\win32_borland\reads
    - c6x\win32_borland\writes
    - c6x\win32_microsoft\reads
    - c6x\win32_microsoft\writes

=========================================================================

API & Tools 1.5.3

  * Create New Project plug-in v. 1.3:
    - now asks what heron module and S/L used, instead of
      asking user to select CDB and CMD files.
    - adds "stub.c" required in S/L 3.2 projects. Includes
      correct heron header file for this source file.

  * Reset plug-in v. 1.3:
    - JTAG reset has been removed from property page, as
      it is impossible to do this (JTAG is under control
      of CCS, plug-in cannot access JTAG).

  * Confidence check:
    - now asks uses whether a HERON1 or 4 is in slot 1, so
      that during install the user can make confchk do the
      right confidence check.

=========================================================================
